<-- previous page Table of Contents Index next page -->

## Octave marks

Octave statements are used to mark notes that are to be played one or more octaves higher or lower than written. An "octave above" statement is used to specify playing higher than written, or "octave below" for playing lower than written. Each item must include a begintime and a text string. The text string is most typically "8va". It will always be printed in 12-point times italics font. If the octave shifting applies to more than a single chord, there should also be a duration specified, reaching to include the last affected note. In this case, Mup will draw a dashed line to mark the span affected. Note that specifying the exact beat of a chord indicates the horizontal center of the chord, so if you want the dashed line to reach a bit past the note, it will be necessary to specify a duration slightly beyond the point of the last chord to be included. Examples:

    1: 2f;g;
    2: 2d+;g;
    3: 2g;ce;
    octave above 1: 2 "8va" til 1m + 1.3;
    bar
    1: 2a;c;
    2: 2f;e;
    3: 4f;;c;;
    octave below 2: 1 "8va";
    octave below 3: 1 "8va" til 2.5; 3 "15" til 4.5;
    bar

<-- previous page Table of Contents Index next page -->