; sysadmin.txt
;
; This is the WaterGate help file
; This file is included by wtrgate.txt
;
; Contents: WtrConf System -> Administrator settings
;

; quick reference:
;
; #topic(reference text)
; #subtopic(reference text)
; #end
; #title(text)
; Space at start of line or #linebreak
; Empty line or #break
; #link(reference)(text)
; #highlight(text) or #hl(text)


;===========================================================================
#topic(System Administrator Settings Editor)
#title(Administrator settings)
This topic is related to the fields found in WtrConf under
System Configuration, Administrator Settings.

In this editor you define the WaterGate Administrator by means
of FTN address or RFC address.

Examples:

  Address type   = Netmail
  FTN username   = Ramon van der Winkel
  FTN address    = 2:280/802.33

  Address type   = E-mail
  E-mail address = ramon@admin.wline.se

#subtopic(SysAdmin AddressType)
#title(Address type)
Select the address type to use when sending a report to the
administrator.
Select the option "Disable" if you do not wish to use the
administrator option.

#subtopic(SysAdmin FTNUserName)
#title(FTN user name)
Enter the Fido user that is to receive the administration
report netmails. The address is filled in in the next field.

#subtopic(SysAdmin FTNAddress)
#title(FTN address)
Enter the Fido address where the administration report netmail
has to be sent.

#subtopic(SysAdmin EmailAddress)
#title(E-mail address)
Enter the e-mail address of the user that is to receive the
administration reports.

#subtopic(SysAdmin SendLog)
#title(Send copy of part added to log)
When set to Yes, the administrator will be sent a copy of the
part of the logfile that was added during the last toss/scan.

#subtopic(SysAdmin CCAFixFwd)
#title(CC: of AreaFix Forward Requests)
When set to Yes, the administrator will be sent a copy of the
message sent to the Area Managers at any of your defined uplinks
when WaterGate requests to connect or disconnect an area.
#end


; end of file sysadmin.txt
